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DORLAND System Control Tech Co., Ltd. has launched the latest Industrial Intrinsically Safe 5G Smartphone Aloha_5G PRO, which adopts advanced 5G technology, intrinsically safe circuit design, powerful appearance, and sturdy body. This phone features a 6.88 "high-definition screen, rear triple camera 64MP main camera+8MP night vision+2MP macro, supports facial recognition, side fingerprint unlocking, and comes standard with NFC. Its waterproof and dustproof performance meets the international IP68 standard.

In addition, it supports Bluetooth, WIFI and other functions to meet the reading and writing needs of various scenarios. We have also configured GPS/Beidou/Galileo/Glonass positioning and other functions suitable for outdoor construction, pipeline inspection, etc. inside the phone, which can be used in conjunction with OA office systems, inspection positioning systems, data acquisition systems and other applications. Especially suitable for harsh environments with hazardous explosions, such as petroleum, chemical, pharmaceutical, oil depots, tank farms, and other hazardous areas with flammable and explosive gases, facilitating timely communication between users, production, and scheduling.

IP Grade: IP68
Ex-marking: Ex ib IIC T4 Gb/Ex ib IIIC T130 ℃ Db
Certificate No.: CCRI 25.7619X

OS: Android 16.0
CPU: MTK Dimensity 7025, 8-core
2*2.5 GHz-Cortex-A78 + 6*2.0 GHz-Cortex-A55
Screen: 6.88 inch HD+120Hz, 720 * 1640, 20.5:9
Memory: 12GB RAM (+Extended RAM: 24GB)
512GB ROM
Extended memory: 2TB T-flash card
Front camera: 32MP front facing camera
Rear camera: rear 64MP (main rear)+8MP (night vision)+2MP (macro)
Battery: 8000mAh, 3.85V
Frequency band: GSM: 2/3/5/8
WCDMA: 1/2/4/5/6/8/19
LTE-TDD: 34/38/39/40/41
LTE-FDD: 1/2/3/4/5/7/8/12/13/17/18/19/20/25/26/28AB/66/71
NR: N1/2/3/5/7/8/12/20/25/28/34/38/39/40/41/48/66/71/77/78
Bluetooth: Bluetooth 5.2
NFC: Supports
Unlocking method: fingerprint recognition+facial recognition
GPS: Beidou Galileo、Glonass、GPS
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	Ex-marking
	Ex ib IIC T4 Gb/ Ex ib IIIC T130℃ Db

	
	Certificate No.
	CCRI 25.7619X

	
	IP Grade
	IP68

	Product overview
	Description

	Product overview
	Weight
	309.5g (including battery)

	
	Dimensions (mm)
	178.4*83.2*11.9mm

	
	OS
	Android 16.0

	Hardware configuration
	Description

	CPU
	Model
	MTK Dimensity 7025

	
	Feature
	8-core
2*2.5 GHz - Cortex-A78
6*2.0 GHz - Cortex-A55

	
	Technology
	6nm

	GPU
	GPU model
	IMG BXM-8-256

	Network
	Network
	GSM+WCDMA+TDD+FDD+NR

	
	Frequency
	GSM: 2/3/5/8
WCDMA: 1/2/4/5/6/8/19
LTE-TDD: 34/38/39/40/41
LTE-FDD: 1/2/3/4/5/7/8/12/13/17/18/19/20/25/26/28AB/66/71
NR: N1/2/3/5/7/8/12/20/25/28/34/38/39/40/41/48/66/71/77/78

	Storage
	Memory
	12GB RAM (+Extended RAM: 24GB)
512GB ROM

	
	SIM card type
	Support Nano Sim card+Nano Sim card / Nano Sim card+TF card

	
	Memory card type
	T-flash card

	
	Expanded memory
	Up to 2TB

	Front Camera 32MP

	Front camera
	Sensor chip
	Sony - IMX616

	
	Software function
	Support facial unlock

	Rear Camera 64MP(Main camera) +8MP(Night vision) +2MP(Macro)

	Main camera
	Sensor chip
	OV64B

	
	Pixel size
	64MP

	
	Flash lamp
	Support

	Night vision camera
	Sensor chip
	Hi-846

	
	Pixel size
	8MP

	
	Flash lamp
	Infrared fill light

	Macro camera
	Sensor chip
	GC02M1

	
	Pixel size
	2MP

	Display
	Size & Technology
	6.88inch  HD+  120Hz

	
	Resolving power
	720*1640

	
	Screen aspect ratio
	20.5:9

	Transmission function
	Navigation
	Support, GPS+GLONASS+Beidou+Galileo

	
	FM
	Support

	
	Wi-Fi
	Support, 802.11 a/b/g/n/ac (2.4G+5G)

	
	Bluetooth
	Support, BT5.2

	
	OTG
	Support

	
	NFC
	Support

	Sensor
	Gravity sensor
	Support

	
	Distance sensor
	Support

	
	Environmental light sensor
	Support

	
	Compass (magnetic)
	Support

	
	Gyroscope
	Support

	Fringeprint Unlock
	Face recognition
	Support

	
	Fingerprint
	Side fingerprint recognition

	Prot
	Earphone port
	Type-C to 3.5mm headphone jack

	
	Charger port
	Type-c

	Physical button
	Power button
	Support

	
	Volume button
	Support

	
	SOS key
	Support

	
	PTT key
	Support

	Battery
	Capacity
	8000mAh

	
	Voltage
	3.85V

	
	Standby time
	1025 hours

	
	Talk time
	146 hours
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Certificate No.: CCRI 25.7619X

Applicant Company: Beijing Dorland System Control Tech Co.,Ltd.
Production: Beijing Dorland System Control Tech Co.,Ltd.
Name of Product: Industrial Intrinsically Safe SG Smartphone
Type of Product: Aloha_5G

Marking: Ex ib I C T4 Gb/Ex ib IIIC T130°C Db
Technical Documents: Q/DLM 010-2025

Drawing No.: Aloha_5G ZZ01

Note(s): See attached sheet

By verifying the drawings, technical documents and checking samples, the product
complies with the following standards currently valid in P.R.China:

GB/T 3836.1-2021, GB/T 3836.4-2021, GB/T 4208-2017

Date of Issue: 11. 13. 2025

Valid till: 11. 12. 2030
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' CONFORMITY CERTIFICATE OF
ccritc EXPLOSION-PROOF ( APPENDIX)

Certificate No.: CCRI 25.7619X

1.Rated voltage DC 3.85V, powered by rechargeable lithium-ion battery packs with
dual protection.

2.0perating environment temperature: -20°C <Ta<+60C.

3.IP code:IP68@1.5m,30min.

4.The suffix "X" indicates that the use of various cable interfaces in hazardous
areas is prohibited, and charging and replacing batteries in hazardous areas is
prohibited; When conducting data transmission or charging, it is necessary to
use specialized connection devices with energy limiting measures that have been
evaluated. Please refer to the instructions for usage precautions.

5.Association inspection report number:2025550883.
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